1. **Contacts:**

**NCAR/EOL Processing and Quality Control:**

Scot Loehrer (NCAR/EOL)

[loehrer@ucar.edu](mailto:loehrer@ucar.edu)

**Original Data Source:**

Donna Holdrige (Argonne National Laboratory)

[djholdridge@anl.gov](mailto:djholdridge@anl.gov)

**2.0 Dataset Overview**

The Department of Energy Atmospheric Radiation Measurement (ARM) Climate Research Facility Southern Great Plains (SGP) site routinely releases radiosondes four times per day (00, 06, 12, and 18 UTC) from its Central Facility located in north central Oklahoma near Lamont (Figure 1; WMO ID 74646). This data set includes the soundings released during the MPEX field phase (15 May to 15 June 2013). A total of 123 quality controlled, high resolution (2-second) soundings are contained in the final MPEX data set.




Figure 1. Location of the ARM SGP Central Facility radiosonde release location.

The Mesoscale Predictability Experiment (MPEX) was a field campaign aimed at investigating if experimental sub-synoptic observations can extend convective-scale predictability and otherwise enhance sill in regional numerical weather prediction over a 6-24 hour time span. The NSF/NCAR Gulfstream-V (GV) aircraft deploying dropsondes was the primary platform used in the experiment. There were also three groups on the ground releasing radiosondes from mobile platforms. Further information on MPEX is available at the MPEX web site: <http://www.eol.ucar.edu/projects/mpex/> and information on MPEX operations are available at the MPEX Field Catalog: <http://catalog.eol.ucar.edu/mpex/>.

**3.0 EOL Sounding Composite (ESC) File Format Description**

The ESC is a columnar ASCII format consisting of 15 header records for each sounding followed by the data records with associated data quality flags.

**3.1 Header Records**

The header records (15 total records) contain a variety of metadata about the sounding (i.e. location, time, radiosonde type, etc). The first five header lines contain information identifying the sounding, and have a rigidly defined form. The following 7 header lines are used for auxiliary information and comments about the sounding, and may vary from dataset to dataset. The last 3 header records contain header information for the data columns. Line 13 holds the field names, line 14 the field units, and line 15 contains dashes ('-' characters) delineating the extent of the field.

The file standard header lines are as follows:

|  |  |  |
| --- | --- | --- |
| **Line** | **Label (padded to 35 char)** | **Contents** |
| 1 | Data Type: | Description of the type and resolution of data |
| 2 | Project ID: | Short name for the field project |
| 3 | Release Site Type/Site ID: | Description of the release site. |
| 4 | Release Location (lon,lat,alt): | Location of the release site. |
| 5 | UTC Release Time (y,m,d,h,m,s): | Time of release. |

The release location is given as:

lon (deg min), lat (deg min), lon (dec. deg), lat (dec. deg), alt (m)

Longitude in deg min is in the format: ddd mm.mm'W where ddd is the number of degrees (with leading zeros if necessary), mm.mm is the decimal number of minutes, and W represents W or E for west or east longitude, respectively. Latitude has the same format as longitude, except there are only two digits for degrees and N or S for north/south latitude.

The time of release is given as: yyyy, mm, dd, hh:nn:ss.

Where yyyy is the year, mm is the month, dd is the day of month, and hh:nn:ss are the UTC hour, minute, and second respectively.

The seven non-standard header lines may contain any label and contents. The labels are padded to 35 characters to match the standard header lines. Records for this data set include the following non-standard header lines:

|  |  |  |
| --- | --- | --- |
| **Line** | **Label (padded to 35 char)** | **Contents** |
| 6 | Sonde Id/Sonde Type: | Radiosonde serial number |
| 7 |  |  |
| 8 |  |  |
| 9 |  |  |
| 10 |  |  |
| 11 |  |  |
| 12 | Nominal Release Time (y,m,d,h,m,s): | Nominal release time |

The nominal release time is 00, 06, 12, or 18 UTC.

**3.2 Data Records**

The data records each contain time from release, pressure, temperature, dew point, relative humidity, U and V wind components, wind speed and direction, ascent rate, balloon position data, altitude, and quality control flags (see the QC code description). Each data line contains 21 fields, separated by spaces, with a total width of 130 characters. The data are right-justified within the fields. All fields have one decimal place of precision, with the exception of latitude and longitude, which have three decimal places of precision. The contents and sizes of the 21 fields that appear in each data record are as follows:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Field** | **Width** | **Format** | **Parameter** | **Units** | **Missing**  **Value** |
| 1 | 6 | F6.1 | Time since release | Seconds | 9999.0 |
| 2 | 6 | F6.1 | Pressure | Millibars | 9999.0 |
| 3 | 5 | F5.1 | Dry-bulb Temperature | Degrees C | 999.0 |
| 4 | 5 | F5.1 | Dew Point Temperature | Degrees C | 999.0 |
| 5 | 5 | F5.1 | Relative Humidity | Percent | 999.0 |
| 6 | 6 | F6.1 | U Wind Comp | m/s | 9999.0 |
| 7 | 6 | F6.1 | V Wind Comp | m/s | 9999.0 |
| 8 | 5 | F5.1 | Wind speed | m/s | 999.0 |
| 9 | 5 | F5.1 | Wind direction | Degrees | 999.0 |
| 10 | 5 | F5.1 | Ascent Rate | m/s | 999.0 |
| 11 | 8 | F8.3 | Longitude | Degrees | 9999.0 |
| 12 | 7 | F7.3 | Latitude | Degrees | 999.0 |
| 13 | 5 | F5.1 | Elevation Angle | Degrees | 999.0 |
| 14 | 5 | F5.1 | Azimuth Angle | Degrees | 999.0 |
| 15 | 7 | F7.1 | Altitude | Meters | 99999.0 |
| 16 | 4 | F4.1 | QC for Pressure | Code | 99.0 |
| 17 | 4 | F4.1 | QC for Temperature | Code | 99.0 |
| 18 | 4 | F4.1 | QC for Humidity | Code | 99.0 |
| 19 | 4 | F4.1 | QC for U Wind | Code | 99.0 |
| 20 | 4 | F4.1 | QC for V Wind | Code | 99.0 |
| 21 | 4 | F4.1 | QC for Ascent Rate | Code | 99.0 |

Fields 16 through 21 contain the data quality flags from the NCAR/Earth Observing Laboratory (EOL) sounding quality control procedures. The data quality flags are defined as follows:

|  |  |
| --- | --- |
| **Code** | **Description** |
| 1.0 | Checked, datum seems physically reasonable. (“GOOD”) |
| 2.0 | Checked, datum seems questionable on a physical basis. (“MAYBE”) |
| 3.0 | Checked, datum seems to be in error. (“BAD”) |
| 4.0 | Checked, datum is interpolated. (“ESTIMATED”) |
| 9.0 | Checked, datum is missing. (“MISSING”) |
| 99.0 | Unchecked (QC information is “missing”.) (“UNCHECKED”) |

**3.3 Data Specifics**

The files contain data calculated at two-second intervals. Complete instrumentation details and specifications are available in the ARM Balloon-Borne Sounding System Handbook available online:

<https://www.arm.gov/publications/tech_reports/handbooks/sonde_handbook.pdf?id=85>

The data are in files by day, so all soundings for a particular day are concatenated into a single file ordered by time. The file naming convention is:

SGP\_C1\_ARM\_yyyymmdd.cls where yyyy is the year, mm is the month, and dd is the day of the month.

The ARM SGP utilized Vaisala RS92-SGP radiosondes with GPS windfinding and the MW-31 DigiCORA-III ground station equipment during MPEX.

**3.4 Sample Data**

The following is a sample of the MPEX ARM high resolution radiosonde data in ESC format.

Data Type: ARM SGP Radiosonde/Ascending

Project ID: MPEX

Release Site Type/Site ID: C1: Lamont, Oklahoma/74646

Release Location (lon,lat,alt): 097 29.40'W, 36 36.60'N, -97.490, 36.610, 315.0

UTC Release Time (y,m,d,h,m,s): 2013, 06, 14, 05:31:00

Sonde Id/Sonde Type: H5013108/Vaisala RS92-SGP with GPS windfinding

/

/

/

/

/

Nominal Release Time (y,m,d,h,m,s):2013, 06, 14, 06:00:00

Time Press Temp Dewpt RH Ucmp Vcmp spd dir Wcmp Lon Lat Ele Azi Alt Qp Qt Qrh Qu Qv QdZ

sec mb C C % m/s m/s m/s deg m/s deg deg deg deg m code code code code code code

------ ------ ----- ----- ----- ------ ------ ----- ----- ----- -------- ------- ----- ----- ------- ---- ---- ---- ---- ---- ----

0.0 977.4 24.6 19.7 74.0 -1.1 2.9 3.1 159.0 0.0 -97.490 36.610 999.0 999.0 315.0 1.0 1.0 1.0 1.0 1.0 99.0

2.0 976.7 24.3 20.6 79.8 -2.4 2.3 3.3 134.0 3.4 -97.490 36.610 999.0 999.0 321.8 1.0 1.0 1.0 1.0 1.0 99.0

4.0 975.7 24.4 20.7 79.9 -2.9 2.6 3.9 132.0 3.9 -97.490 36.610 999.0 999.0 330.7 1.0 1.0 1.0 1.0 1.0 99.0

6.0 974.6 24.5 20.7 79.1 -3.4 3.2 4.7 133.0 4.2 -97.490 36.610 999.0 999.0 340.5 1.0 1.0 1.0 1.0 1.0 99.0

**3.5 Station List**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **ID** | **Site Name** | **State** | **Longitude** | **Latitude** | **Elev (m)** |
| 74646 | Central Facility | OK | -97.490 | 36.610 | 315 |

**4.0 Data Quality Control Procedures**

1. Each sounding was converted from its original format (NetCDF) into the ESC format described above.
2. Each sounding was passed through a set of automated data quality checks which included basic gross limit checks as well as rate of change checks. This is further described in Section 4.1.
3. Each sounding was visually examined utilizing the NCAR/EOL XQC sounding quality control software. This is further described in Section 4.2.

**4.1 Automated Data Quality Checks**

This data set was passed through a set of automated data quality checks. This procedure includes both gross limit checks on all parameters as well as rate-of-change checks on temperature, pressure, and ascent rate. A version of these checks is described in Loehrer et al. (1996) and Loehrer et al. (1998).

**4.1.1 Gross Limit Checks**

These checks were conducted on each sounding and the data quality flags in the ESC files were adjusted as appropriate. Only the data point under examination was flagged. All checks also produced warning messages that specified the location of the problem and the severity of the issue. These warning messages where then summarized statistically and examined to determine any consistent issues.

For this data set NCAR/EOL conducted the following gross limit checks. In the table P = pressure, T = temperature, RH = relative humidity, U = U wind component, V = V wind component, B= bad, and Q = questionable.

|  |  |  |  |
| --- | --- | --- | --- |
| **Parameter** | **Check** | **Parameter(s) Flagged** | **Flag Applied** |
| Pressure | <0 or > 1050 | P | B |
| Altitude | < 0 or >40000 | P, T, RH | Q |
| Temperature | < -90 or > 45 | T | B |
| Dew Point | < -99.9 or > 33  > T | RH  T, RH | Q  Q |
| Wind Speed | < 0 or > 100  > 150 | U, V  U, V | Q  B |
| U Wind | < 0 or > 100  > 150 | U  U | Q  B |
| V Wind | < 0 or > 100  > 150 | V  V | Q  B |
| Wind Direction | < 0 or > 360 | U, V | B |
| Ascent Rate | < -10 or > 10 | P, T, RH | Q |

**4.1.2 Vertical Consistency Checks**

These checks were conducted on each sounding and the data quality flags in the ESC files were adjusted as appropriate. These checks were started at the surface and compared each neighboring data record. In the case of checks that ensured that the values increased/decreased as expected, only the data point under examination was flagged. However, for the other checks, all of the data points used in the examination were flagged. All items within the table are as previously defined. All checks also produced warning messages that specified the location of the problem and the severity of the issue. These warning messages where then summarized statistically and examined to determine any consistent issues.

|  |  |  |  |
| --- | --- | --- | --- |
| **Parameter** | **Check** | **Parameter(s) Flagged** | **Flag Applied** |
| Time | Decreasing/equal | None | None. |
| Altitude | Decreasing/equal | P, T, RH | Q |
| Pressure | Increasing/equal  > 1mb/s or < -1mb/s  > 2mb/s or < -2mb/s | P, T, TH  P, T, TH  P, T, TH | Q  Q  B |
| Temperature | < -15oC/km  < -30oC/km  > 50oC/km  > 100oC/km | P, T, RH  P, T, RH  P, T, RH  P, T, RH | Q  B  Q  B |
| Ascent Rate | > 3m/s or < -3m/s  > 5m/s or < -5m/s | P  P | Q  B |

**4.2 Visual Data Quality Checks**

Each sounding was visually examined using the NCAR/EOL XQC sounding data quality control software. This software allows the user to view a skew-t/log-p diagram of each sounding and apply data quality flags as appropriate. The user can zoom in on sections of soundings for detailed examination and can adjust the data quality flags for an individual point, sections of soundings, or entire soundings for each parameter individually. The software also allows the user to override the quality flags applied by the automated procedure.

**4.3 Data Quality Issues of Note**

The data quality control procedures outlined above allows us to identify and, in some cases, resolve issues that could potentially impact research performed using these data sets. The following issues were noted in these soundings.

1. One file (27 May 2013 at 1120 UTC) contained only a surface data record and was not included in the final data set. There was no second release so no sounding data are available at the 1200 UTC nominal time on 27 May.
2. Significant wet-bulbing (superadiabatic layers near cloud top) was evident for short periods and the temperature data were flagged as questionable in the following soundings:

19 May at 1124 UTC

7 June at 2342 UTC.

1. The relative humidity data at upper levels in a few soundings are quite noisy and were flagged as questionable:

29 May at 1130 UTC (above ~255mb)

31 May at 1133 UTC (above ~185mb)

2 June at 0524 UTC (above ~150mb)

1. In two of those same soundings (29 and 31 May) there was also a period at upper levels where the temperature and relative humidity data were oddly smooth and were flagged as questionable (100-70mb on 29 May and above 100mb on 31 May).

**5.0 References**

Loehrer, S. M., T. A. Edmands, and J. A. Moore, 1996: TOGA COARE upper-air sounding data archive: development and quality control procedures. Bull. Amer. Meteor. Soc., 77, 2651-2671.

Loehrer, S. M., S. F. Williams, and J. A. Moore, 1998: Results from UCAR/JOSS quality control of atmospheric soundings from field projects. Preprints, Tenth Symposium on Meteorological Observations and Instrumentation, Phoenix, AZ, Amer. Meteor. Soc., 1-6.