1. **Contacts:**

**NCAR/EOL Processing and Quality Control:**

Scot Loehrer (NCAR/EOL)

[loehrer@ucar.edu](mailto:loehrer@ucar.edu)

**Data Provider:**

ARM User Facility

<http://dx.doi.org/%2010.5439/1150271>

1. **Dataset Overview**

The Department of Energy/Atmospheric Radiation Measurement (DOE/ARM) program operated a radiosonde system on-board the RSV Aurora Australis as part of the Measurements of Aerosols, Radiation, and Clouds over the Southern Ocean (MARCUS) field campaign. The Australis conducted servicing cruises to Davis, Casey, and Mawson Stations on the Antarctica coast from its base at Hobart, Tasmania. Radiosondes were released every six hours (00, 06, 12, 18 UTC) during these cruises. This data set includes only those soundings that were released during the SOCARATES (Southern Ocean Clouds, Radiation, Aerosol Transport Experimental Study) field phase (1 January – 28 February 2018). A total of 208 2-second vertical resolution radiosondes are included in this data set.




Figure 1. Locations of the MARCUS RSV Aurora Australis radiosonde release locations from 1 January to 28 February 2018.

**Project Overview**

The **Southern Ocean Clouds, Radiation, Aerosol Transport Experimental Study (SOCRATES)** is a research program to improve our understanding of clouds, aerosols, air-sea exchanges, and their interactions over the Southern Ocean. SOCRATES utilized the NSF/NCAR GV HIAPER aircraft based out of Hobart, Tasmania. There were additional projects occurring at the same time that were cooperating with SOCRATES, these included the DOE/ARM MARCUS (Measurements of Aerosols, Radiation, and Clouds over the Southern Ocean) project which used the RSV Aurora Australis, the DOE/ARM MICRE (Macquarie Island Cloud and Radiation Experiment) and the Australian CAPRICORN (Clouds, Aerosols, Precipitation Radiation and atmospherIc Composition Over the southeRN ocean) project which utilized the RV Investigator. Further information on VORTEX-SE is available at the SOCARTES web site at NCAR/EOL: <https://www.eol.ucar.edu/field_projects/socrates> and information on the SOCRATES deployments is available at the SOCRATES Field Catalog: <http://catalog.eol.ucar.edu/socrates>.

1. **EOL Sounding Composite (ESC) File Format Description**

The ESC is a columnar ASCII format consisting of 15 header records for each sounding followed by the data records with associated data quality flags.

**3.1 Header Records**

The header records (15 total records) contain a variety of metadata about the sounding (i.e. location, time, radiosonde type, etc). The first five header lines contain information identifying the sounding, and have a rigidly defined form. The following 7 header lines are used for auxiliary information and comments about the sounding, and may vary from dataset to dataset. The last 3 header records contain header information for the data columns. Line 13 holds the field names, line 14 the field units, and line 15 contains dashes ('-' characters) delineating the extent of the field.

The file standard header lines are as follows:

|  |  |  |
| --- | --- | --- |
| **Line** | **Label (padded to 35 char)** | **Contents** |
| 1 | Data Type: | Description of the type and resolution of data |
| 2 | Project ID: | Short name for the field project |
| 3 | Release Site Type/Site ID: | Description of the release site. |
| 4 | Release Location (lon,lat,alt): | Location of the release site. |
| 5 | UTC Release Time (y,m,d,h,m,s): | Time of release. |

The release location is given as:

lon (deg min), lat (deg min), lon (dec. deg), lat (dec. deg), alt (m)

Longitude in deg min is in the format: ddd mm.mm'W where ddd is the number of degrees (with leading zeros if necessary), mm.mm is the decimal number of minutes, and W represents W or E for west or east longitude, respectively. Latitude has the same format as longitude, except there are only two digits for degrees and N or S for north/south latitude.

The time of release is given as: yyyy, mm, dd, hh:nn:ss.

Where yyyy is the year, mm is the month, dd is the day of month, and hh:nn:ss are the UTC hour, minute, and second respectively.

The seven non-standard header lines may contain any label and contents. The labels are padded to 35 characters to match the standard header lines. Records for this data set include the following non-standard header lines:

|  |  |  |
| --- | --- | --- |
| **Line** | **Label (padded to 35 char)** | **Contents** |
| 6 | Radiosonde Serial Number |  |
| 7 | Radiosonde Type |  |
| 8 | Ground Station Software |  |
| 9 |  |  |
| 10 |  |  |

**3.2 Data Records**

The data records each contain time from release, pressure, temperature, dew point, relative humidity, U and V wind components, wind speed and direction, ascent rate, balloon position data, altitude, and quality control flags (see the QC code description). Each data line contains 21 fields, separated by spaces, with a total width of 130 characters. The data are right-justified within the fields. All fields have one decimal place of precision, with the exception of latitude and longitude, which have three decimal places of precision. The contents and sizes of the 21 fields that appear in each data record are as follows:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Field** | **Width** | **Format** | **Parameter** | **Units** | **Missing**  **Value** |
| 1 | 6 | F6.1 | Time since release | Seconds | 9999.0 |
| 2 | 6 | F6.1 | Pressure | Millibars | 9999.0 |
| 3 | 5 | F5.1 | Dry-bulb Temperature | Degrees C | 999.0 |
| 4 | 5 | F5.1 | Dew Point Temperature | Degrees C | 999.0 |
| 5 | 5 | F5.1 | Relative Humidity | Percent | 999.0 |
| 6 | 6 | F6.1 | U Wind Comp | m/s | 9999.0 |
| 7 | 6 | F6.1 | V Wind Comp | m/s | 9999.0 |
| 8 | 5 | F5.1 | Wind speed | m/s | 999.0 |
| 9 | 5 | F5.1 | Wind direction | Degrees | 999.0 |
| 10 | 5 | F5.1 | Ascent Rate | m/s | 999.0 |
| 11 | 8 | F8.3 | Longitude | Degrees | 9999.0 |
| 12 | 7 | F7.3 | Latitude | Degrees | 999.0 |
| 13 | 5 | F5.1 | Elevation Angle | Degrees | 999.0 |
| 14 | 5 | F5.1 | Mixing Ratio | g/kg | 999.0 |
| 15 | 7 | F7.1 | Geopotential Height | Meters | 99999.0 |
| 16 | 4 | F4.1 | QC for Pressure | Code | 99.0 |
| 17 | 4 | F4.1 | QC for Temperature | Code | 99.0 |
| 18 | 4 | F4.1 | QC for Humidity | Code | 99.0 |
| 19 | 4 | F4.1 | QC for U Wind | Code | 99.0 |
| 20 | 4 | F4.1 | QC for V Wind | Code | 99.0 |
| 21 | 4 | F4.1 | QC for Ascent Rate | Code | 99.0 |

Fields 16 through 21 contain the data quality flags from the NCAR/Earth Observing Laboratory (EOL) sounding quality control procedures. The data quality flags are defined as follows:

|  |  |
| --- | --- |
| **Code** | **Description** |
| 1.0 | Checked, datum seems physically reasonable. (“GOOD”) |
| 2.0 | Checked, datum seems questionable on a physical basis. (“MAYBE”) |
| 3.0 | Checked, datum seems to be in error. (“BAD”) |
| 4.0 | Checked, datum is interpolated. (“ESTIMATED”) |
| 9.0 | Checked, datum is missing. (“MISSING”) |
| 99.0 | Unchecked (QC information is “missing”.) (“UNCHECKED”) |

**3.3 Data Specifics**

The data are in files by day, so all soundings for a particular day are concatenated into a single file ordered by time. The file naming convention is:

MARCUS\_yyyymmdd.cls where yyyy is the year, mm is the month, and dd is the day of the month.

DOE/ARM utilized the Vaisala RS92-SGP and Vaisala DigiCORA 3.64 ground station.

**3.4 Sample Data**

The following is a sample of the MSU mobile high resolution radiosonde data in ESC format.

Data Type: DOE/ARM Sounding Data/Ascending

Project ID: SOCRATES - MARCUS

Release Site Type/Site ID: RSV Aurora Australis/VNAA

Release Location (lon,lat,alt): 110 32.40'E, 66 16.20'S, 110.540, -66.270, 17.0

UTC Release Time (y,m,d,h,m,s): 2017, 12, 31, 23:59:00

Radiosonde Serial Number: N2313930

Radiosonde Type: Vaisala RS92-SGP

Ground Station Software: Vaisala DigiCORA 3.64

/

/

/

Nominal Release Time (y,m,d,h,m,s):2018, 01, 01, 00:00:00

Time Press Temp Dewpt RH Ucmp Vcmp spd dir Wcmp Lon Lat Ele Azi Alt Qp Qt Qrh Qu Qv QdZ

sec mb C C % m/s m/s m/s deg m/s deg deg deg deg m code code code code code code

------ ------ ----- ----- ----- ------ ------ ----- ----- ----- -------- ------- ----- ----- ------- ---- ---- ---- ---- ---- ----

0.0 985.8 -1.3 -2.9 89.0 2.6 2.4 3.5 227.0 0.0 110.540 -66.270 999.0 999.0 17.0 2.0 2.0 2.0 99.0 99.0 99.0

2.0 983.7 -1.5 -10.6 50.0 2.6 2.4 3.5 227.0 8.5 110.540 -66.270 999.0 999.0 34.0 2.0 2.0 2.0 99.0 99.0 99.0

4.0 982.2 -1.7 -7.5 64.2 2.5 2.3 3.4 228.0 7.2 110.540 -66.270 999.0 999.0 45.9 99.0 99.0 99.0 99.0 99.0 99.0

**3.5 Station List**

This was a mobile system.

**4.0 Data Quality Control Procedures**

1. NCAR/EOL converted each sounding from its original format into the ESC format described above. The station elevation was derived from Google Earth using the release location. The geopotential height, dew point, and wind components were derived common methods.
2. NCAR/EOL passed each sounding through a set of automated data quality checks which included basic gross limit checks as well as rate of change checks. This is further described in Section 4.1.
3. NCAR/EOL visually examined each sounding utilizing the NCAR/EOL XQC sounding quality control software. This is further described in Section 4.2.

**4.1 Automated Data Quality Checks**

This data set was passed through a set of automated data quality checks. This procedure includes both gross limit checks on all parameters as well as rate-of-change checks on temperature, pressure, and ascent rate. A version of these checks is described in Loehrer et al. (1996) and Loehrer et al. (1998).

**4.1.1 Gross Limit Checks**

These checks were conducted on each sounding and the data quality flags in the ESC files were adjusted as appropriate. Only the data point under examination was flagged. All checks also produced warning messages that specified the location of the problem and the severity of the issue. These warning messages where then summarized statistically and examined to determine any consistent issues.

For this data set NCAR/EOL conducted the following gross limit checks. In the table P = pressure, T = temperature, RH = relative humidity, U = U wind component, V = V wind component, B= bad, and Q = questionable.

|  |  |  |  |
| --- | --- | --- | --- |
| **Parameter** | **Check** | **Parameter(s) Flagged** | **Flag Applied** |
| Pressure | <0 or > 1050 | P | B |
| Altitude | < 0 or >40000 | P, T, RH | Q |
| Temperature | < -90 or > 45 | T | B |
| Dew Point | < -99.9 or > 33  > T | RH  T, RH | Q  Q |
| Wind Speed | < 0 or > 100  > 150 | U, V  U, V | Q  B |
| U Wind | < 0 or > 100  > 150 | U  U | Q  B |
| V Wind | < 0 or > 100  > 150 | V  V | Q  B |
| Wind Direction | < 0 or > 360 | U, V | B |
| Ascent Rate | < -10 or > 10 | P, T, RH | Q |

**4.1.2 Vertical Consistency Checks**

These checks were conducted on each sounding and the data quality flags in the ESC files were adjusted as appropriate. These checks were started at the surface and compared each neighboring data record. In the case of checks that ensured that the values increased/decreased as expected, only the data point under examination was flagged. However, for the other checks, all of the data points used in the examination were flagged. All items within the table are as previously defined. All checks also produced warning messages that specified the location of the problem and the severity of the issue. These warning messages where then summarized statistically and examined to determine any consistent issues.

|  |  |  |  |
| --- | --- | --- | --- |
| **Parameter** | **Check** | **Parameter(s) Flagged** | **Flag Applied** |
| Time | Decreasing/equal | None | None. |
| Altitude | Decreasing/equal | P, T, RH | Q |
| Pressure | Increasing/equal  > 1mb/s or < -1mb/s  > 2mb/s or < -2mb/s | P, T, TH  P, T, TH  P, T, TH | Q  Q  B |
| Temperature | < -15oC/km  < -30oC/km  > 50oC/km  > 100oC/km | P, T, RH  P, T, RH  P, T, RH  P, T, RH | Q  B  Q  B |
| Ascent Rate | > 3m/s or < -3m/s  > 5m/s or < -5m/s | P  P | Q  B |

**4.2 Visual Data Quality Checks**

Each sounding was visually examined using the NCAR/EOL XQC sounding data quality control software. This software allows the user to view a skew-t/log-p diagram of each sounding and apply data quality flags as appropriate. The user can zoom in on sections of soundings for detailed examination and can adjust the data quality flags for an individual point, sections of soundings, or entire soundings for each parameter individually. The software also allows the user to override the quality flags applied by the automated procedure.

**4.3 Data Quality Issues of Note**

The data quality control procedures outlined above allows us to identify and, in some cases, resolve issues that could potentially impact research performed using these data sets. The following issues were noted in these soundings.

In most soundings the initial radiosonde humidity values are low and take a few seconds to acclimatize to the environmental values.

**201801272330 –** Surface wind value incorrect

**201802041131 –** Surface wind value incorrect

**201802162334** – No GPS/wind data

**201802201730** – Surface wind value incorrect

**5.0 References**

Loehrer, S. M., T. A. Edmands, and J. A. Moore, 1996: TOGA COARE upper-air sounding data archive: development and quality control procedures. Bull. Amer. Meteor. Soc., 77, 2651-2671.

Loehrer, S. M., S. F. Williams, and J. A. Moore, 1998: Results from UCAR/JOSS quality control of atmospheric soundings from field projects. Preprints, Tenth Symposium on Meteorological Observations and Instrumentation, Phoenix, AZ, Amer. Meteor. Soc., 1-6.