1. **Contacts:**

**NCAR/EOL Processing and Quality Control:**

Scot Loehrer (NCAR/EOL)

[loehrer@ucar.edu](mailto:loehrer@ucar.edu)

**Original Data Source:**

Kevin Vermeesch (kevin.c.vermeesch@nasa.gov)

1. **Dataset Overview**

The University of Maryland – Baltimore County (UMBC) and the Naval Postgraduate School (NPS) released radiosondes at the PECAN Fixed PISA (PECAN Integrated Sounding Array) 2 site in Greensburg, Kansas (Figure 1). These releases were conducted during PECAN operations. This data set includes the quality controlled PECAN Fixed PISA 2 UMBC (31 May – 16 July 2015) and NPS (11-12 July 2015) soundings released for the PECAN field phase. A total of 124 (114 UMBC and 10 NPS) quality-controlled, high vertical resolution (1-second) soundings are contained in the final PECAN data set.




Figure 1. Location of the PECAN Fixed PISA 2 (Greensburg, KS) radiosonde site.

1. **Project Overview**

Plains Elevated Convection At Night (PECAN) was a multi-agency project designed to advance the understanding of continental, nocturnal, warm season precipitation. It focused on nocturnal convection in conditions over the central United States plains states with a stable boundary layer (SBL), a nocturnal low-level jet and the largest convective available potential energy located above the SBL. Three aircraft (University of Wyoming King Air, NOAA P-3, and NASA DC-8) as well as a large array of fixed and mobile ground instrumentation were deployed out of Kansas from 1 June to 15 July 2015. Further information on PECAN is available at the PECAN web site: <https://www.eol.ucar.edu/field_projects/pecan> and information on PECAN operations is available at the PECAN Field Catalog: <http://catalog.eol.ucar.edu/pecan>.

1. **EOL Sounding Composite (ESC) File Format Description**

The ESC is a columnar ASCII format consisting of 15 header records for each sounding followed by the data records with associated data quality flags.

**3.1 Header Records**

The header records (15 total records) contain a variety of metadata about the sounding (i.e. location, time, radiosonde type, etc). The first five header lines contain information identifying the sounding, and have a rigidly defined form. The following 7 header lines are used for auxiliary information and comments about the sounding, and may vary from dataset to dataset. The last 3 header records contain header information for the data columns. Line 13 holds the field names, line 14 the field units, and line 15 contains dashes ('-' characters) delineating the extent of the field.

The file standard header lines are as follows:

|  |  |  |
| --- | --- | --- |
| **Line** | **Label (padded to 35 char)** | **Contents** |
| 1 | Data Type: | Description of the type and resolution of data |
| 2 | Project ID: | Short name for the field project |
| 3 | Release Site Type/Site ID: | Description of the release site. |
| 4 | Release Location (lon,lat,alt): | Location of the release site. |
| 5 | UTC Release Time (y,m,d,h,m,s): | Time of release. |

The release location is given as:

lon (deg min), lat (deg min), lon (dec. deg), lat (dec. deg), alt (m)

Longitude in deg min is in the format: ddd mm.mm'W where ddd is the number of degrees (with leading zeros if necessary), mm.mm is the decimal number of minutes, and W represents W or E for west or east longitude, respectively. Latitude has the same format as longitude, except there are only two digits for degrees and N or S for north/south latitude.

The time of release is given as: yyyy, mm, dd, hh:nn:ss.

Where yyyy is the year, mm is the month, dd is the day of month, and hh:nn:ss are the UTC hour, minute, and second respectively.

The seven non-standard header lines may contain any label and contents. The labels are padded to 35 characters to match the standard header lines. Records for this data set include the following non-standard header lines:

|  |  |  |
| --- | --- | --- |
| **Line** | **Label (padded to 35 char)** | **Contents** |
| 6 | Radiosonde Type | Type of Radiosonde |
| 7 | Radiosonde Serial Number |  |

**3.2 Data Records**

The data records each contain time from release, pressure, temperature, dew point, relative humidity, U and V wind components, wind speed and direction, ascent rate, balloon position data, altitude, and quality control flags (see the QC code description). Each data line contains 21 fields, separated by spaces, with a total width of 130 characters. The data are right-justified within the fields. All fields have one decimal place of precision, with the exception of latitude and longitude, which have three decimal places of precision. The contents and sizes of the 21 fields that appear in each data record are as follows:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Field** | **Width** | **Format** | **Parameter** | **Units** | **Missing**  **Value** |
| 1 | 6 | F6.1 | Time since release | Seconds | 9999.0 |
| 2 | 6 | F6.1 | Pressure | Millibars | 9999.0 |
| 3 | 5 | F5.1 | Dry-bulb Temperature | Degrees C | 999.0 |
| 4 | 5 | F5.1 | Dew Point Temperature | Degrees C | 999.0 |
| 5 | 5 | F5.1 | Relative Humidity | Percent | 999.0 |
| 6 | 6 | F6.1 | U Wind Comp | m/s | 9999.0 |
| 7 | 6 | F6.1 | V Wind Comp | m/s | 9999.0 |
| 8 | 5 | F5.1 | Wind speed | m/s | 999.0 |
| 9 | 5 | F5.1 | Wind direction | Degrees | 999.0 |
| 10 | 5 | F5.1 | Ascent Rate | m/s | 999.0 |
| 11 | 8 | F8.3 | Longitude | Degrees | 9999.0 |
| 12 | 7 | F7.3 | Latitude | Degrees | 999.0 |
| 13 | 5 | F5.1 | Elevation Angle | Degrees | 999.0 |
| 14 | 5 | F5.1 | Azimuth Angle | Degrees | 999.0 |
| 15 | 7 | F7.1 | Altitude | Meters | 99999.0 |
| 16 | 4 | F4.1 | QC for Pressure | Code | 99.0 |
| 17 | 4 | F4.1 | QC for Temperature | Code | 99.0 |
| 18 | 4 | F4.1 | QC for Humidity | Code | 99.0 |
| 19 | 4 | F4.1 | QC for U Wind | Code | 99.0 |
| 20 | 4 | F4.1 | QC for V Wind | Code | 99.0 |
| 21 | 4 | F4.1 | QC for Ascent Rate | Code | 99.0 |

Fields 16 through 21 contain the data quality flags from the NCAR/Earth Observing Laboratory (EOL) sounding quality control procedures. The data quality flags are defined as follows:

|  |  |
| --- | --- |
| **Code** | **Description** |
| 1.0 | Checked, datum seems physically reasonable. (“GOOD”) |
| 2.0 | Checked, datum seems questionable on a physical basis. (“MAYBE”) |
| 3.0 | Checked, datum seems to be in error. (“BAD”) |
| 4.0 | Checked, datum is interpolated. (“ESTIMATED”) |
| 9.0 | Checked, datum is missing. (“MISSING”) |
| 99.0 | Unchecked (QC information is “missing”.) (“UNCHECKED”) |

**3.3 Data Specifics**

The files contain data at one-second intervals.

For most of PECAN, UMBC released their radiosondes at the PECAN FP2 site. On 11-12 July NPS released their radiosondes at FP2. The UMBC radiosondes have “UMBC/Ascending” as the Data Type in the data file headers and the NPS radiosondes have “NPS/Ascending”.

The data are in files by day, so all soundings for a particular day are concatenated into a single file ordered by time. The file naming convention is:

GREEN\_ORG\_yyyymmdd.cls where yyyy is the year, mm is the month, and dd is the day of the month. ORG specifies NPS or UMBC radiosondes.

The UMBC group utilized Vaisala RS41 radiosondes and the NPS group utilized InterMet Systems iMet1 radiosondes. Both radiosondes used GPS for windfinding during PECAN.

**3.4 Sample Data**

The following is a sample of the FP2 UMBC high resolution radiosonde data in ESC format. The format is the same for the NPS radiosondes.

Data Type: UMBC/Ascending

Project ID: PECAN

Release Site Type/Site ID: FP2 GREEN/Greensburg, KS

Release Location (lon,lat,alt): 099 16.57'W, 37 36.38'N, -99.276, 37.606, 680.0

UTC Release Time (y,m,d,h,m,s): 2015, 05, 31, 15:36:00

Radiosonde Type: Vaisala RS41

Radiosonde Serial Number: L0930386

/

/

/

/

Nominal Release Time (y,m,d,h,m,s):2015, 05, 31, 15:36:00

Time Press Temp Dewpt RH Ucmp Vcmp spd dir Wcmp Lon Lat Ele Azi Alt Qp Qt Qrh Qu Qv QdZ

sec mb C C % m/s m/s m/s deg m/s deg deg deg deg m code code code code code code

------ ------ ----- ----- ----- ------ ------ ----- ----- ----- -------- ------- ----- ----- ------- ---- ---- ---- ---- ---- ----

0.0 943.1 18.3 10.9 62.0 0.7 2.0 2.1 199.0 999.0 -99.276 37.606 0.0 0.0 680.0 99.0 99.0 99.0 99.0 99.0 9.0

1.4 942.4 17.9 11.6 66.5 1.1 1.4 1.8 219.0 4.5 -99.276 37.606 27.1 47.8 686.5 2.0 2.0 2.0 99.0 99.0 99.0

2.4 941.9 17.4 11.2 66.8 1.2 1.3 1.8 222.8 4.7 -99.276 37.606 32.0 40.7 691.2 2.0 2.0 2.0 99.0 99.0 99.0

**3.5 Station List**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Site ID** | **WMO ID** | **Site Name** | **Latitude** | **Longitude** | **Elev (m)** |
| FP2 | N/A | Greensburg, KS | 37.606N | 99.276W | 680 |

**4.0 Data Quality Control Procedures**

1. Each sounding was converted from its original format into the ESC format described above.
2. Each sounding was passed through a set of automated data quality checks which included basic gross limit checks as well as rate of change checks. This is further described in Section 4.1.
3. Each sounding was visually examined utilizing the NCAR/EOL XQC sounding quality control software. This is further described in Section 4.2.

**4.1 Automated Data Quality Checks**

This data set was passed through a set of automated data quality checks. This procedure includes both gross limit checks on all parameters as well as rate-of-change checks on temperature, pressure, and ascent rate. A version of these checks is described in Loehrer et al. (1996) and Loehrer et al. (1998).

**4.1.1 Gross Limit Checks**

These checks were conducted on each sounding and the data quality flags in the ESC files were adjusted as appropriate. Only the data point under examination was flagged. All checks also produced warning messages that specified the location of the problem and the severity of the issue. These warning messages where then summarized statistically and examined to determine any consistent issues.

For this data set NCAR/EOL conducted the following gross limit checks. In the table P = pressure, T = temperature, RH = relative humidity, U = U wind component, V = V wind component, B= bad, and Q = questionable.

|  |  |  |  |
| --- | --- | --- | --- |
| **Parameter** | **Check** | **Parameter(s) Flagged** | **Flag Applied** |
| Pressure | <0 or > 1050 | P | B |
| Altitude | < 0 or >40000 | P, T, RH | Q |
| Temperature | < -90 or > 45 | T | B |
| Dew Point | < -99.9 or > 33  > T | RH  T, RH | Q  Q |
| Wind Speed | < 0 or > 100  > 150 | U, V  U, V | Q  B |
| U Wind | < 0 or > 100  > 150 | U  U | Q  B |
| V Wind | < 0 or > 100  > 150 | V  V | Q  B |
| Wind Direction | < 0 or > 360 | U, V | B |
| Ascent Rate | < -10 or > 10 | P, T, RH | Q |

**4.1.2 Vertical Consistency Checks**

These checks were conducted on each sounding and the data quality flags in the ESC files were adjusted as appropriate. These checks were started at the surface and compared each neighboring data record. In the case of checks that ensured that the values increased/decreased as expected, only the data point under examination was flagged. However, for the other checks, all of the data points used in the examination were flagged. All items within the table are as previously defined. All checks also produced warning messages that specified the location of the problem and the severity of the issue. These warning messages where then summarized statistically and examined to determine any consistent issues.

|  |  |  |  |
| --- | --- | --- | --- |
| **Parameter** | **Check** | **Parameter(s) Flagged** | **Flag Applied** |
| Time | Decreasing/equal | None | None. |
| Altitude | Decreasing/equal | P, T, RH | Q |
| Pressure | Increasing/equal  > 1mb/s or < -1mb/s  > 2mb/s or < -2mb/s | P, T, TH  P, T, TH  P, T, TH | Q  Q  B |
| Temperature | < -15oC/km  < -30oC/km  > 50oC/km  > 100oC/km | P, T, RH  P, T, RH  P, T, RH  P, T, RH | Q  B  Q  B |
| Ascent Rate | > 3m/s or < -3m/s  > 5m/s or < -5m/s | P  P | Q  B |

**4.2 Visual Data Quality Checks**

Each sounding was visually examined using the NCAR/EOL XQC sounding data quality control software. This software allows the user to view a skew-t/log-p diagram of each sounding and apply data quality flags as appropriate. The user can zoom in on sections of soundings for detailed examination and can adjust the data quality flags for an individual point, sections of soundings, or entire soundings for each parameter individually. The software also allows the user to override the quality flags applied by the automated procedure.

**4.3 Data Quality Issues of Note**

The data quality control procedures outlined above allows us to identify and, in some cases, resolve issues that could potentially impact research performed using these data sets. The following issues were noted in these soundings.

**UMBC soundings**

**201506080306** – Wetbulbing from ~587-568mb and 396-370mb. The temperature and RH data are bad above 180mb.

**201506220000** – The RH data are noisy throughout the sounding (particularly below 653mb and above 553mb), flagged bad.

**201506220100** – The sounding contains no data from the surface to 103mb.

**201506220606** – The sounding contains no data from the surface to 805mb.

**201506260300** – Wetbulbing from ~667-660mb.

**201507070009** – Slow ascent sounding.

**201507070600** – Slow ascent sounding.

**201507100702** – No wind data from ~903mb-622mb and ~463-311mb. Temperature and RH data look interpolated during much of this time, flagged questionable.

**NPS soundings**

**201507102359** – Wetbulbing ~762-700mb.

**201507110557** – The temperature data are noisy above 134mb.

**201507110756** – The RH data are noisy above 156mb.

**201507112159** – The RH data are noisy above 158mb.

**5.0 References**

Loehrer, S. M., T. A. Edmands, and J. A. Moore, 1996: TOGA COARE upper-air sounding data archive: development and quality control procedures. Bull. Amer. Meteor. Soc., 77, 2651-2671.

Loehrer, S. M., S. F. Williams, and J. A. Moore, 1998: Results from UCAR/JOSS quality control of atmospheric soundings from field projects. Preprints, Tenth Symposium on Meteorological Observations and Instrumentation, Phoenix, AZ, Amer. Meteor. Soc., 1-6.